skeinforge_application.skeinforge_plugins.craft_plugins.fill ($Date: 2008/28/04 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/fabmetheus/skeinforge_application/skeinforge_plugins/craft_plugins/fill.py

Previous / Next / Contents

`
Fill is a script to fill the perimeters of a gcode file.
The fill manual page is at:
http://www.bitsfrombytes.com/wiki/index.php?title=Skeinforge_Fill
Allan Ecker aka The Masked Retriever has written the "Skeinforge Quicktip: Fill" at:
http://blog.thingiverse.com/2009/07/21/mysteries-of-skeinforge-fill/
Operation
Settings
Diaphragm
Diaphragm Period
Diaphragm Thickness
Extra Shells
Extra Shells on Alternating Solid Layers
Extra Shells on Base
Extra Shells on Sparse Layer
Grid
Grid Circle Separation over Perimeter Width
Grid Extra Overlap
Grid Junction Separation over Octogon Radius At End
Grid Junction Separation over Octogon Radius At Middle
Grid Junction Separation Band Height
Infill
Infill Pattern
Grid Circular
Grid Hexagonal
Grid Rectangular
Line
Infill Begin Rotation
Infill Odd Layer Extra Rotation
Infill Begin Rotation Repeat
Infill Perimeter Overlap
Infill Solidity
Interior Infill Density over Exterior Density
Infill Width over Thickness
Solid Surface Thickness
Thread Sequence Choice
Infill > Loops > Perimeter
Infill > Perimeter > Loops
Loops > Infill > Perimeter
Loops > Perimeter > Infill
Perimeter > Infill > Loops
Perimeter > Loops > Infill
Examples
`

## Operation

The default 'Activate Fill' checkbox is off. When it is on, the functions described below will work, when it is off, the functions will not be called.

## Settings

### Diaphragm

The diaphragm is a solid group of layers, at regular intervals. It can be used with a sparse infill to give the object watertight, horizontal compartments and/or a higher shear strength.

#### Diaphragm Period

Default is one hundred.
Defines the number of layers between diaphrams.

#### Diaphragm Thickness

Default is zero, because the diaphragm feature is rarely used.
Defines the number of layers the diaphram is composed of.

### Extra Shells

The shells interior perimeter loops. Adding extra shells makes the object stronger & heavier.

#### Extra Shells on Alternating Solid Layers

Default is two.
Defines the number of extra shells, on the alternating solid layers.

#### Extra Shells on Base

Default is one.
Defines the number of extra shells on the bottom, base layer and every even solid layer after that. Setting this to a different value than the "Extra Shells on Alternating Solid Layers" means the infill pattern will alternate, creating a strong interleaved bond even if the perimeter loop shrinks.

#### Extra Shells on Sparse Layer

Default is one.
Defines the number of extra shells on the sparse layers. The solid layers are those at the top & bottom, and wherever the object has a plateau or overhang, the sparse layers are the layers in between.

### Grid

#### Grid Circle Separation over Perimeter Width

Default is 0.2.
Defines the ratio of the amount the grid circle is inset over the perimeter width, the default is zero. With a value of zero the circles will touch, with a value of one two threads could be fitted between the circles.

#### Grid Extra Overlap

Default is 0.1.
Defines the amount of extra overlap added when extruding the grid to compensate for the fact that when the first thread going through a grid point is extruded, since there is nothing there yet for it to connect to it will shrink extra.

#### Grid Junction Separation over Octogon Radius At End

Default is zero.
Defines the ratio of the amount the grid square is increased in each direction over the extrusion width at the end. With a value of one or so the grid pattern will have large squares to go with the octogons.

#### Grid Junction Separation over Octogon Radius At Middle

Default is zero.
Defines the increase at the middle. If this value is different than the value at the end, the grid would have an accordion pattern, which would give it a higher shear strength.

#### Grid Junction Separation Band Height

Default is ten.
Defines the height of the bands of the accordion pattern.

### Infill

#### Infill Pattern

Default is 'Line', since it is quicker to generate and does not add extra movements for the extruder. The grid pattern has extra diagonal lines, so when choosing a grid option, set the infill solidity to 0.2 or less so that there is not too much plastic and the grid generation time, which increases with the third power of solidity, will be reasonable.

##### Grid Circular

When selected, the infill will be a grid of separated circles. Because the circles are separated, the pattern is weak, it only provides support for the top layer threads and some strength in the z direction. The flip side is that this infill does not warp the object, the object will get warped only by the walls.
Because this pattern turns the extruder on and off often, it is best to use a stepper motor extruder.

##### Grid Hexagonal

When selected, the infill will be a hexagonal grid. Because the grid is made with threads rather than with molding or milling, only a partial hexagon is possible, so the rectangular grid pattern is stronger.

##### Grid Rectangular

When selected, the infill will be a funky octogon square honeycomb like pattern which gives the object extra strength.

##### Line

When selected, the infill will be made up of lines.

#### Infill Begin Rotation

Default is forty five degrees, giving a diagonal infill.
Defines the amount the infill direction of the base and every second layer thereafter is rotated.

#### Infill Odd Layer Extra Rotation

Default is ninety degrees, making the odd layer infill perpendicular to the base layer.
Defines the extra amount the infill direction of the odd layers is rotated compared to the base layer.

#### Infill Begin Rotation Repeat

Default is one, giving alternating cross hatching.
Defines the number of layers that the infill begin rotation will repeat. With a value higher than one, the infill will go in one direction more often, giving the object more strength in one direction and less in the other, this is useful for beams and cantilevers.

#### Infill Perimeter Overlap

Default is 0.15.
Defines the amount the infill overlaps the perimeter over the average of the perimeter and infill width. The higher the value the more the infill will overlap the perimeter, and the thicker join between the infill and the perimeter. If the value is too high, the join will be so thick that the nozzle will run plow through the join below making a mess, also when it is above 0.45 fill may not be able to create infill correctly. If you want to stretch the infill a lot, set 'Path Stretch over Perimeter Width' in stretch to a high value.

#### Infill Solidity

Default is 0.2.
Defines the solidity of the infill, this is the most important setting in fill. A value of one means the infill lines will be right beside each other, resulting in a solid, strong, heavy shape which takes a long time to extrude. A low value means the infill will be sparse, the interior will be mosty empty space, the object will be weak, light and quick to build.

#### Interior Infill Density over Exterior Density

Default is 0.9.
Defines the ratio of the infill density of the interior over the infill density of the exterior surfaces. The exterior should have a high infill density, so that the surface will be strong and watertight. With the interior infill density a bit lower than the exterior, the plastic will not fill up higher than the extruder nozzle. If the interior density is too high that could happen, as Nophead described in the Hydraraptor "Bearing Fruit" post at:
http://hydraraptor.blogspot.com/2008/08/bearing-fruit.html

#### Infill Width over Thickness

Default is 1.5.
Defines the ratio of the infill width over the layer thickness. The higher the value the wider apart the infill will be and therefore the sparser the infill will be.

### Solid Surface Thickness

Default is three.
Defines the number of solid layers that are at the bottom, top, plateaus and overhang. With a value of zero, the entire object will be composed of a sparse infill, and water could flow right through it. With a value of one, water will leak slowly through the surface and with a value of three, the object could be watertight. The higher the solid surface thickness, the stronger and heavier the object will be.

### Thread Sequence Choice

The 'Thread Sequence Choice' is the sequence in which the threads will be extruded. There are three kinds of thread, the perimeter threads on the outside of the object, the loop threads aka inner shell threads, and the interior infill threads.
The default choice is 'Perimeter > Loops > Infill', which the default stretch parameters are based on. If you change from the default sequence choice setting of perimeter, then loops, then infill, the optimal stretch thread parameters would also be different. In general, if the infill is extruded first, the infill would have to be stretched more so that even after the filament shrinkage, it would still be long enough to connect to the loop or perimeter. The six sequence combinations follow below.

#### Infill > Loops > Perimeter

#### Infill > Perimeter > Loops

#### Loops > Infill > Perimeter

#### Loops > Perimeter > Infill

#### Perimeter > Infill > Loops

#### Perimeter > Loops > Infill

## Examples

The following examples fill the file Screw Holder Bottom.stl. The examples are run in a terminal in the folder which contains Screw Holder Bottom.stl and fill.py.
> python fill.py
This brings up the fill dialog.
> python fill.py Screw Holder Bottom.stl
The fill tool is parsing the file:
Screw Holder Bottom.stl
..
The fill tool has created the file:
.. Screw Holder Bottom_fill.gcode
> python
Python 2.5.1 (r251:54863, Sep 22 2007, 01:43:31)
[GCC 4.2.1 (SUSE Linux)] on linux2
Type "help", "copyright", "credits" or "license" for more information.
>>> import fill
>>> fill.main()
This brings up the fill dialog.
>>> fill.writeOutput('Screw Holder Bottom.stl')
The fill tool is parsing the file:
Screw Holder Bottom.stl
..
The fill tool has created the file:
.. Screw Holder Bottom_fill.gcode

Previous / Next / Contents

Modules
`` |  |
__init__ fabmetheus_utilities.archive fabmetheus_utilities.euclidean fabmetheus_utilities.fabmetheus_tools.fabmetheus_interpret | fabmetheus_utilities.gcodec fabmetheus_utilities.intercircle math fabmetheus_utilities.settings | skeinforge_application.skeinforge_utilities.skeinforge_craft skeinforge_application.skeinforge_utilities.skeinforge_polyfile skeinforge_application.skeinforge_utilities.skeinforge_profile sys | fabmetheus_utilities.geometry.solids.trianglemesh

Classes
`` |  | FillRepository FillSkein RotatedLayer YIntersectionPath
class FillRepository
`` | `A class to handle the fill settings.`
| Methods defined here: __init__(self) `Set the default settings, execute title & settings fileName.` execute(self) `Fill button has been clicked.`
class FillSkein
`` | `A class to fill a skein of extrusions.`
| Methods defined here: __init__(self) addFill(self, layerIndex) `Add fill to the carve layer.` addGcodeFromThreadZ(self, thread, z) `Add a gcode thread to the output.` addGrid(self, arounds, fillLoops, gridPointInsetX, layerIndex, paths, pixelTable, reverseRotation, surroundingCarves, width) `Add the grid to the infill layer.` addGridCircle(self, center, infillPaths, layerRotation, pixelTable, rotatedLoops, startRotation, width) `Add circle to the grid.` addGridLinePoints(self, begin, end, gridPoints, gridRotationAngle, offset, y) `Add the segments of one line of a grid to the infill.` addRemainingGridPoints(self, arounds, gridPointInsetX, gridPointInsetY, gridPoints, isBothOrNone, paths, pixelTable, width) `Add the remaining grid points to the grid point list.` addRotatedCarve(self, layerIndex, reverseRotation, surroundingCarves) `Add a rotated carve to the surrounding carves.` addThreadsBridgeLayer(self, rotatedLayer, surroundingLoops) `Add the threads, add the bridge end & the layer end tag.` addToThread(self, location) `Add a location to thread.` getAreaChange(self, area, layerIndex) `Get the difference between the area of the carve at the layer index and the given area.` getCarveArea(self, layerIndex) `Get the area of the carve.` getCraftedGcode(self, repository, gcodeText) `Parse gcode text and store the bevel gcode.` getGridPoints(self, fillLoops, reverseRotation) `Get the grid points.` getGridPointsByLoops(self, gridRotationAngle, loops) `Get the grid points by loops.` getIsDensitySolidityPositive(self) `Determine if the infillSolidity and infillInteriorDensityOverExteriorDensity are both positive.` getLayerRotation(self, layerIndex) `Get the layer rotation.` getNextGripXStep(self, gridXStep) `Get the next grid x step, increment by an extra one every three if hexagonal grid is chosen.` isGridToBeExtruded(self) `Determine if the grid is to be extruded.` isPointInsideLineSegments(self, gridPoint) `Is the point inside the line segments of the loops.` linearMove(self, splitLine) `Add a linear move to the thread.` parseInitialization(self) `Parse gcode initialization and store the parameters.` parseLine(self, lineIndex) `Parse a gcode line and add it to the fill skein.` setGridVariables(self, repository) `Set the grid variables.`
class RotatedLayer
`` | `A rotated layer.`
| Methods defined here: __init__(self, z) __repr__(self) `Get the string representation of this RotatedLayer.`
class YIntersectionPath
`` | `A class to hold the y intersection position, the loop which it intersected and the point index of the loop which it intersected.`
| Methods defined here: __init__(self, pathIndex, pointIndex, y) `Initialize from the path, point index, and y.` __repr__(self) `Get the string representation of this y intersection.` getPath(self, paths) `Get the path from the paths and path index.` getPointIndexPlusOne(self) `Get the point index plus one.`

Functions
`` |  | addAroundGridPoint(arounds, gridPoint, gridPointInsetX, gridPointInsetY, gridPoints, gridSearchRadius, isBothOrNone, isDoubleJunction, isJunctionWide, paths, pixelTable, width) `Add the path around the grid point.` addLoop(infillWidth, infillPaths, loop, rotationPlaneAngle) `Add simplified path to fill.` addPath(infillWidth, infillPaths, path, rotationPlaneAngle) `Add simplified path to fill.` addPathIndexFirstSegment(gridPixel, pathIndexTable, pixelTable, segmentFirstPixel) `Add the path index of the closest segment found toward the second segment.` addPathIndexSecondSegment(gridPixel, pathIndexTable, pixelTable, segmentSecondPixel) `Add the path index of the closest segment found toward the second segment.` addPointOnPath(path, pathIndex, pixelTable, point, pointIndex, width) `Add a point to a path and the pixel table.` addPointOnPathIfFree(path, pathIndex, pixelTable, point, pointIndex, width) `Add the closest point to a path, if the point added to a path is free.` addSparseEndpoints(doubleExtrusionWidth, endpoints, fillLine, horizontalSegmentLists, infillSolidity, removedEndpoints, solidSurfaceThickness, surroundingXIntersections) `Add sparse endpoints.` addSparseEndpointsFromSegment(doubleExtrusionWidth, endpoints, fillLine, horizontalSegmentLists, infillSolidity, removedEndpoints, segment, solidSurfaceThickness, surroundingXIntersections) `Add sparse endpoints from a segment.` addYIntersectionPathToList(pathIndex, pointIndex, y, yIntersection, yIntersectionPaths) `Add the y intersection path to the y intersection paths.` compareDistanceFromCenter(self, other) `Get comparison in order to sort y intersections in ascending order of distance from the center.` comparePointIndexDescending(self, other) `Get comparison in order to sort y intersections in descending order of point index.` createExtraFillLoops(radius, shouldExtraLoopsBeAdded, surroundingLoop) `Create extra fill loops.` createFillForSurroundings(radius, shouldExtraLoopsBeAdded, surroundingLoops) `Create extra fill loops for surrounding loops.` getAdditionalLength(path, point, pointIndex) `Get the additional length added by inserting a point into a path.` getClosestOppositeIntersectionPaths(yIntersectionPaths) `Get the close to center paths, starting with the first and an additional opposite if it exists.` getCraftedText(fileName, gcodeText='', repository=None) `Fill the inset file or gcode text.` getCraftedTextFromText(gcodeText, repository=None) `Fill the inset gcode text.` getExtraFillLoops(loops, radius) `Get extra loops between inside and outside loops.` getKeyIsInPixelTableAddValue(key, pathIndexTable, pixelTable) `Determine if the key is in the pixel table, and if it is and if the value is not None add it to the path index table.` getNewRepository() `Get the repository constructor.` getNonIntersectingGridPointLine(gridPointInsetX, isJunctionWide, paths, pixelTable, yIntersectionPath, width) `Get the points around the grid point that is junction wide that do not intersect.` getPlusMinusSign(number) `Get one if the number is zero or positive else negative one.` getWithLeastLength(path, point) `Insert a point into a path, at the index at which the path would be shortest.` getYIntersectionInsideYSegment(segmentFirstY, segmentSecondY, beginComplex, endComplex, x) `Get the y intersection inside the y segment if it does, else none.` insertGridPointPair(gridPoint, gridPointInsetX, gridPoints, isJunctionWide, paths, pixelTable, yIntersectionPath, width) `Insert a pair of points around the grid point is is junction wide, otherwise inset one point.` insertGridPointPairWithLinePath(gridPoint, gridPointInsetX, gridPoints, isJunctionWide, linePath, paths, pixelTable, yIntersectionPath, width) `Insert a pair of points around the grid point is is junction wide, otherwise inset one point.` insertGridPointPairs(gridPoint, gridPointInsetX, gridPoints, intersectionPathFirst, intersectionPathSecond, isBothOrNone, isJunctionWide, paths, pixelTable, width) `Insert a pair of points around a pair of grid points.` isAddedPointOnPathFree(path, pixelTable, point, pointIndex, width) `Determine if the point added to a path is intersecting the pixel table or the path.` isAddedPointOnPathIntersectingPath(begin, path, point, pointIndex) `Determine if the point added to a path is intersecting the path by checking line intersection.` isIntersectingLoopsPaths(loops, paths, pointBegin, pointEnd) `Determine if the segment between the first and second point is intersecting the loop list.` isPointAddedAroundClosest(pixelTable, layerExtrusionWidth, paths, removedEndpointPoint, width) `Add the closest removed endpoint to the path, with minimal twisting.` isSegmentAround(aroundSegments, segment) `Determine if there is another segment around.` isSegmentCompletelyInAnIntersection(segment, xIntersections) `Add sparse endpoints from a segment.` isSegmentInX(segment, xFirst, xSecond) `Determine if the segment overlaps within x.` isSharpCorner(beginComplex, centerComplex, endComplex) `Determine if the three complex points form a sharp corner.` isSidePointAdded(pixelTable, closestPath, closestPathIndex, closestPointIndex, layerExtrusionWidth, removedEndpointPoint, width) `Add side point along with the closest removed endpoint to the path, with minimal twisting.` main() `Display the fill dialog.` removeEndpoints(pixelTable, layerExtrusionWidth, paths, removedEndpoints, aroundWidth) `Remove endpoints which are added to the path.` setIsOutside(yCloseToCenterPath, yIntersectionPaths) `Determine if the yCloseToCenterPath is outside.` writeOutput(fileName='') `Fill an inset gcode file.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __date__ = '$Date: 2008/28/04 $' __license__ = 'GPL 3.0' absolute_import = _Feature((2, 5, 0, 'alpha', 1), (2, 7, 0, 'alpha', 0), 16384)

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)