English, see below...
Diese Dateien sind für den Anycubic Kobra X.

1. Filamenthalter V1
2. Filamenthalter V2
3. Abfallbox

Alle Dateien müssen mit Tree-Support gedruckt werden(bis auf die Klammer für die Abfallbox).

Druckempfehlung:
PLA/PETG
0,2 -0,4mm Layerhöhe
20% Infill

Für die Filamenthalter gibt es jeweils zwei Versionen.
Einmal komplett und einmal in zwei Teile geschnitten.
Die geschnitten Teile müssen zusammengesteckt und verklebt werden. Die Steckstifte haben enge Toleranzen. Sollten Sie zu groß sein, einfach mit etwas Schleifpapier dünner machen.

--------------------------------

These files are for the Anycubic Kobra X.

1. Filament Holder V1

2. Filament Holder V2
3. Waste Bin

All files must be printed with tree supports (except for the waste bin clip).

Printing recommendation:
PLA/PETG
0.2–0.4 mm layer height
20% infill

There are two versions of each filament holder: one complete and one cut into two parts.

The cut parts must be assembled and glued together. The pins have tight tolerances. If they are too large, simply thin them with some sandpaper.