skeinforge_application.skeinforge_plugins.craft_plugins.unpause ($Date: 2008/21/04 $) | index /home/enrique/Desktop/backup/babbleold/script/reprap/fabmetheus/skeinforge_application/skeinforge_plugins/craft_plugins/unpause.py

Previous / Next / Contents

`
The unpause script is based on the Shane Hathaway's patch to speed up a line segment to compensate for the delay of the microprocessor. The description is at:
http://shane.willowrise.com/archives/delay-compensation-in-firmware/
The unpause manual page is at:
http://www.bitsfrombytes.com/wiki/index.php?title=Skeinforge_Unpause
Operation
Settings
Delay
Maximum Speed
Examples
`

## Operation

The default 'Activate Unpause' checkbox is off. When it is on, the functions described below will work, when it is off, the functions will not be called.

## Settings

### Delay

Default is 28 milliseconds, which Shane found for the Arduino.
Defines the delay on the microprocessor that will be at least partially compensated for.

### Maximum Speed

Default is 1.3.
Defines the maximum amount that the feed rate will be sped up to, compared to the original feed rate.

## Examples

The following examples unpause the file Screw Holder Bottom.stl. The examples are run in a terminal in the folder which contains Screw Holder Bottom.stl and unpause.py.
> python unpause.py
This brings up the unpause dialog.
> python unpause.py Screw Holder Bottom.stl
The unpause tool is parsing the file:
Screw Holder Bottom.stl
..
The unpause tool has created the file:
.. Screw Holder Bottom_unpause.gcode
> python
Python 2.5.1 (r251:54863, Sep 22 2007, 01:43:31)
[GCC 4.2.1 (SUSE Linux)] on linux2
Type "help", "copyright", "credits" or "license" for more information.
>>> import unpause
>>> unpause.main()
This brings up the unpause dialog.
>>> unpause.writeOutput('Screw Holder Bottom.stl')
The unpause tool is parsing the file:
Screw Holder Bottom.stl
..
The unpause tool has created the file:
.. Screw Holder Bottom_unpause.gcode

Previous / Next / Contents

Modules
`` |  |
__init__ fabmetheus_utilities.archive fabmetheus_utilities.euclidean | fabmetheus_utilities.fabmetheus_tools.fabmetheus_interpret fabmetheus_utilities.gcodec fabmetheus_utilities.intercircle | math fabmetheus_utilities.settings skeinforge_application.skeinforge_utilities.skeinforge_craft | skeinforge_application.skeinforge_utilities.skeinforge_polyfile sys

Classes
`` |  | UnpauseRepository UnpauseSkein
class UnpauseRepository
`` | `A class to handle the unpause settings.`
| Methods defined here: __init__(self) `Set the default settings, execute title & settings fileName.` execute(self) `Unpause button has been clicked.`
class UnpauseSkein
`` | `A class to unpause a skein of extrusions.`
| Methods defined here: __init__(self) getCraftedGcode(self, gcodeText, repository) `Parse gcode text and store the unpause gcode.` getUnpausedArcMovement(self, line, splitLine) `Get an unpaused arc movement.` getUnpausedLinearMovement(self, line, splitLine) `Get an unpaused linear movement.` getUnpausedMovement(self, distance, line, splitLine) `Get an unpaused movement.` parseInitialization(self) `Parse gcode initialization and store the parameters.` parseLine(self, line) `Parse a gcode line.`

Functions
`` |  | getCraftedText(fileName, gcodeText, repository=None) `Unpause a gcode linear move file or text.` getCraftedTextFromText(gcodeText, repository=None) `Unpause a gcode linear move text.` getNewRepository() `Get the repository constructor.` getSelectedPlugin(repository) `Get the selected plugin.` main() `Display the unpause dialog.` writeOutput(fileName='') `Unpause a gcode linear move file.`

Data
`` |  | __author__ = 'Enrique Perez (perez_enrique@yahoo.com)' __date__ = '$Date: 2008/21/04 $' __license__ = 'GPL 3.0' absolute_import = _Feature((2, 5, 0, 'alpha', 1), (2, 7, 0, 'alpha', 0), 16384)

Author
`` |  | Enrique Perez (perez_enrique@yahoo.com)