Bergman 1-100 PolskiFiat 508/iii w family

Please remember: CC BY-SA-NC license.

PolskiFiat 508/iiiw (2 door)              -  civilian sedan, sometimes used as command car.
PolskiFiat 508/iiiw (4 door)              -  civilian sedan, sometimes used as command car.

PolskiFiat 508/iiiw delivery van          -  civilian only delivery van.

PolskiFiat 508/iiiw panel van (civilian)  -  civilian panel van. (different bumper). Post Office.
PolskiFiat 508/iiiw panel van (military)  -  military panel van. Police, ambulance.

PolskiFiat 508/iiiw pickup (civilian)     -  civilian pickup. (different bumper, no tools) Open and closed versions.
PolskiFiat 508/iiiw pickup (military)     -  military pickup. (tools) Open and closed versions.
PolskiFiat 508/iiiw pickup ambulance      -  military field ambulance pickup. One stretcher could be carried beside the driver.

PolskiFiat 508/iiiw Lazik (early)         -  military field car. Early version has square boot, two spares on rear face. 
PolskiFiat 508/iiiw Lazik (late)          -  military field car. Late version has rounded boot, two spares inset in mudguards.

                                             Lazik late (open) has option of BAR fitted between front seats. BAR also supplied as a seperate part.
                                             Both Laziks have a closed option, optimised for both SLA and FDM. SLA versions are one piece.
                                             FDM versions have seperate roof, and gearsticks omitted. Simple versions with solid windscreen also provided.
                                             Both Laziks have option of window up or down. Simple versions with solid windscreen also supplied. 
                                             FDM versions with gearsticks omitted are supplied and strongly recommended.
                                             

All vehicles printed sitting on their wheels.
Roofs for Lazik printed best for me lying on their sides, with the rearview mirror pointing up.
Suggest that BAR is printed sitting on its side, lying flat on the print bed.

If you have trouble clearing out Lazik steering wheel, suggest cutting it off right away and gluing it back in place later. Makes support removal much easier.

